[bookmark: _ai_b1]Installation instructions
[bookmark: _ai_b2]Turn the power off
Switch off the circuit at the breaker before you start. Installation must be done by a qualified electrician.
[bookmark: _ai_b3]In the box
· [bookmark: _ai_b4]SP-24 panel
· Driver box with 1.5 m lead
· 4 safety cables
· This guide
[bookmark: _ai_b5]Tools you need
[bookmark: _ai_b6]Wire strippers, a 3 mm flat screwdriver, a ladder and a voltage tester.
[bookmark: _ai_b7]Steps
1. [bookmark: _ai_b8]Remove a ceiling tile and check the opening is 600 x 1200 mm.
2. Fix the safety cables to the structure above.
a. Use the supplied anchors in concrete.
b. Keep the cables slack by about 50 mm.
3. Connect the supply to the driver box: L (brown), N (blue), earth (green/yellow).
4. Lift the panel into the grid and clip the safety cables to the frame.
5. Restore power and test all modes.
[bookmark: _ai_b9][image: ]
Figure 1: Clipping the safety cable to the frame
[bookmark: _ai_b10]Wiring
	[bookmark: _ai_b11]Terminal
	Wire colour
	Connect to

	L
	Brown
	Live

	N
	Blue
	Neutral

	PE
	Green/yellow
	Earth

	DA+ / DA-
	Grey / white
	DALI bus (polarity free)


[bookmark: _ai_b12]Leave 300 mm of slack in the supply so the panel can be lowered for service.
[bookmark: _ai_b13]Troubleshooting
	[bookmark: _ai_b14]Problem
	What to check

	Panel stays off
	Breaker, supply wiring and the driver LED

	Flicker when dimmed
	Dimmer compatibility; use 0-10 V or DALI
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