Assembly guide  |  Bookcase BK-5
Five-Shelf Bookcase: Assembly Guide
Flat-pack bookcase, 800 W x 300 D x 1900 H mm. Two people, about 45 minutes.
Before you start
Clear a floor area of about 2 x 2 m and lay the carton flat. Open it on the long side and lay the panels on the carton so the finished faces are not scratched. Check every part against the list below before you begin; if anything is missing, stop and contact the retailer.
	Tip-over hazard
This bookcase must be fixed to the wall with the restraint strap supplied. Children have been injured by furniture tipping over.



Parts
	Part
	Description
	Size (mm)
	Qty

	A
	Side panel, pre-drilled
	1900 x 300 x 18
	2

	B
	Fixed shelf
	764 x 290 x 18
	2

	C
	Bottom shelf with plinth
	764 x 290 x 18
	1

	D
	Top panel
	800 x 300 x 18
	1

	E
	Back panel, hardboard
	1880 x 780 x 3
	1

	F
	Adjustable shelf
	760 x 280 x 18
	2



Hardware
	Code
	Item
	Qty

	H1
	Cam lock, 15 mm
	12

	H2
	Cam bolt, M6 x 34
	12

	H3
	Wood dowel, 8 x 30
	16

	H4
	Shelf pin, 5 mm
	8

	H5
	Back-panel nail, 20 mm
	28

	H6
	Wall restraint strap with screws
	1



Tools you need: a Phillips screwdriver (PH2), a small hammer, and a tape measure. A drill is only needed for fixing to the wall.


Step 1: Dowels and cam bolts
Lay both side panels (A) on the carton with the pre-drilled holes facing up. Tap a dowel (H3) into each of the 16 small holes. Screw a cam bolt (H2) into each threaded insert by hand until the shoulder is flush with the panel.
Step 2: Shelves into one side
Fit the bottom shelf (C) and the two fixed shelves (B) onto the dowels of one side panel. Drop a cam lock (H1) into each round hole in the shelves with the arrow pointing at the bolt, then turn it half a turn clockwise until it pulls the joint tight.
[image: ]
Figure 1. Turn the cam lock until it grips the bolt. Do not over-tighten.
Step 3: Second side and top
With a second person holding the shelves upright, lower the other side panel onto the dowels and lock the cams. Fit the top panel (D) last.
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Figure 2. Exploded view: sides A, fixed shelves B, bottom shelf C, top D and back panel E.
Step 4: Square the frame and fit the back
Lay the frame on its front edge.
Measure both diagonals. Push the long corner until the two diagonals are equal (within 2 mm).
Place the back panel (E) in the rebate with the white side facing the front.
Nail it every 150 mm with the 20 mm nails (H5), starting at the corners.
Step 5: Stand up and fix to the wall
Stand the bookcase upright against the wall. Fix the restraint strap (H6) to the top panel and to the wall using a fixing suitable for your wall (the screws supplied suit timber studs only). Insert the shelf pins (H4) at the heights you want and place the adjustable shelves (F).
	Shelf
	Maximum load

	Fixed shelf B
	25 kg

	Adjustable shelf F
	15 kg

	Bottom shelf C
	30 kg



Care
Wipe with a damp cloth and dry immediately. Do not use solvent cleaners.
Check and re-tighten the cam locks after the first month.
Keep away from radiators and direct sun to avoid warping and fading.
Keep these instructions for future reference.
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